**Mobility Lift Instructions.**

**Going Up.**

1. **Call Lift / Open Door.** Press & hold the down button till it illuminates red. Lift door will open automatically.
2. **Close door.** Press and Hold the UP Button till it illuminates red. Lift door will close automatically.
3. **To operate Lift from inside.** Press and hold the up button until the lift completely ascends. Lift Door will open automatically.
4. **To Operate Lift from outside.** Press and hold the up button until it illuminates red. Lift will ascend and door will open automatically.
5. **Close Door.** Door will close automatically after a few moments. But can be closed by pressing the down button till it illuminates red.

**Going Down.**

1. **Call Lift / Open Door.** Press & hold the UP button till it illuminates red. Lift door will open automatically.
2. **Close door.** Press and Hold the Down Button till it illuminates red. Lift door will close automatically.
3. **To operate Lift from inside.** Press and hold the DOWN button until the lift completely ascends. Lift Door will open automatically.
4. **To Operate Lift from outside.** Press and hold the DOWN button until it illuminates red. Lift will ascend and door will open automatically.
5. **Close Door.** Door will close automatically after a few moments. But can be closed by pressing the UP button till it illuminates red.

PLEASE NOTE Lift will not function if any of the emergency stops are pressed. There are 4 emergency stop buttons in total, 1 at the bottom of the lift, 2 inside the lift and 1 at the top of the lift. To disengage the stops, please twist clockwise. All buttons will flash red if any of the Emergency Stops are engaged.